Note:
Before installing the executive program, proposed closing anti-virus software first strongly! 
Because in the course of installing, some antivirus software will delete or forbid the materials installed, 
make the installation fail or cut off.

Version Revision Record
==================================================================
V1.2.9 (2022.04.29)
*. Supported Hardware model:
   -Emulator: HY17S58-DK0x (development kit)
   -Emulator: HY17S68-DK0x (development kit)
   -Writer: HY10000-WK08x (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Fixed the include files of HY17P58 series for HAO calibration.
   -Fixed an error message that appeared when extern repeated the name.
==================================================================
V1.2.8 (2021.09.06)
*. Supported Hardware model:
   -Emulator: HY17S58-DK0x (development kit)
   -Emulator: HY17S68-DK0x (development kit)
   -Writer: HY10000-WK08x (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Update the include files, INC files, Info files & Demo Code.
   -Update HY17S68-L216_ICE Board_A18039 from V02 to V03
   -Update the schematic of HY17S58-IM02 ICE board.
   -Delete the schematics of HY17S58-IM01 & HY17S68-IM01 ICE board.
   -Add the schematic of HY17S58-IM02 ICE board.
   -Add the schematic of HY17S68-IM02 ICE board.
   -Add the schematic of HY17S68-IM03 ICE board.
   -Add HY17P6x series products.
   -Fixed the issue that "ADC output bits" 's GUI of HY17P6x don't work normally.
   -Fixed the issue that Main area's BIE of HY17P6x don't work normally.
   -Fix the HY17P4X/5X mem files to turn on TPS calibration function.
==================================================================
V1.1 (2020.06.08)
*. Supported Hardware model:
   -Emulator: HY17S58-DK0x Series (development kit)
   -Writer: HY10000-WK08C (programming kit)
   -Writer: HY10000-WK08D (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Update Info. file for HY17P48.
   -Speed up the programming time.
   -Fixed the issue that BIE can not be displayed.
   -Unify the include's *.mem files to C:\HYCON\INCLUDE
   -Update the schematic of HY17S58-L128 ICE Board.
   -Update the demo codes.
==================================================================
V1.0 (2019.01.31)
*. Supported Hardware model:
   -Emulator: HY17S58-DK01 (development kit)
   -Writer: HY10000-WK08C (programming kit)
   -Writer: HY10000-WK08D (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -First Edition
